Interface              IP-Address      OK? Method Status                Protocol
 
FastEthernet0/0        unassigned      YES unset  administratively down down
 
FastEthernet1/0        unassigned      YES unset  administratively down down
 
Serial2/0              172.17.0.1      YES manual up                    up
 
Serial3/0              unassigned      YES unset  administratively down down
 
FastEthernet4/0        unassigned      YES unset  administratively down down
 
FastEthernet5/0        unassigned      YES unset  administratively down down