Interface              IP-Address      OK? Method Status                Protocol
 
FastEthernet0/0        172.16.0.1      YES manual up                    up
 
FastEthernet1/0        192.168.0.1     YES manual up                    up
 
Serial2/0              unassigned      YES unset  administratively down down
 
Serial3/0              unassigned      YES unset  administratively down down
 
FastEthernet4/0        unassigned      YES unset  administratively down down
 
FastEthernet5/0        unassigned      YES unset  administratively down down
 
Modem6/0               unassigned      YES unset  down                  down
 
FastEthernet7/0        unassigned      YES unset  up                    down